EXTERNAL PORTS
These are the external ports defined in the MHS file.
Attributes Key The attributes are obtained from the SIGIS and IOB_STATE parameters set on the PORT in the MHS file CLK indicates Clock ports, (SIGIS = CLK) INTR indicates Interrupt ports,(SIGIS = INTR) RESET indicates Reset ports, (SIGIS = RST) BUF or REG Indicates ports that instantiate or infer IOB primitives, (IOB_STATE = BUF or REG)
# | NAME | DIR | [LSB:MSB] | SIG | ATTRIBUTES
| fpga_0_RS232_RX_pin | I | 1 | fpga_0_RS232_RX |
| fpga_0_RS232_TX_pin | O | 1 | fpga_0_RS232_TX |
| fpga_0_LEDs_8Bit_GPIO_d_out_pin | O | 0:7 | fpga_0_LEDs_8Bit_GPIO_d_out |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_ODT_pin | O | 0:0 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_ODT |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_A_pin | O | 12:0 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_A |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_BA_pin | O | 1:0 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_BA |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_CAS_N_pin | O | 1 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_CAS_N |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_CKE_pin | O | 1 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_CKE |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_CS_N_pin | O | 1 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_CS_N |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_RAS_N_pin | O | 1 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_RAS_N |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_WE_N_pin | O | 1 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_WE_N |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_DM_pin | O | 3:0 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_DM |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_DQS | IO | 3:0 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_DQS |  |  | # | NAME | DIR | [LSB:MSB] | SIG | ATTRIBUTES
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_DQS_N | IO | 3:0 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_DQS_N |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_DQ | IO | 31:0 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_DQ |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_CK_pin | O | 1:0 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_CK |
| fpga_0_DDR2_SDRAM_16Mx32_DDR2_CK_N_pin | O | 1:0 | fpga_0_DDR2_SDRAM_16Mx32_DDR2_CK_N |
| sys_clk_pin | I | 1 | dcm_clk_s | CLK
| sys_rst_pin | I | 1 | sys_rst_s | RESET
| fpga_0_SysACE_CompactFlash_SysACE_CLK_pin | I | 1 | fpga_0_SysACE_CompactFlash_SysACE_CLK |
| fpga_0_SysACE_CompactFlash_SysACE_MPA_pin | O | 6:0 | fpga_0_SysACE_CompactFlash_SysACE_MPA |
| fpga_0_SysACE_CompactFlash_SysACE_MPD_pin | IO | 15:0 | fpga_0_SysACE_CompactFlash_SysACE_MPD |
| fpga_0_SysACE_CompactFlash_SysACE_CEN_pin | O | 1 | fpga_0_SysACE_CompactFlash_SysACE_CEN |
| fpga_0_SysACE_CompactFlash_SysACE_OEN_pin | O | 1 | fpga_0_SysACE_CompactFlash_SysACE_OEN |
| fpga_0_SysACE_CompactFlash_SysACE_WEN_pin | O | 1 | fpga_0_SysACE_CompactFlash_SysACE_WEN |
| fpga_0_SysACE_CompactFlash_SysACE_MPIRQ_pin | I | 1 | fpga_0_SysACE_CompactFlash_SysACE_MPIRQ |